,Catalog Number##other##,Product Description##other##,Fixture Type##other##,Type Lens##other##,3_Lamp##other##,4_Lamp##other##,6_Lamp##other##,Lamp##other##,Watt##other##,Wattage##other##,Efficacy##other##,Voltage##other##,Boxed Weight##other##,Photometric Web File##other##
HEF265-2L-TM-U,HEF265-2L-TM-U,"32 Watt Rapid Start Medium Bi-Pin T8, 265mA, 48""",Two Lamp Fixture,Tempered Glass,0,0,0,T8,32,64,80,277,37 lbs.,HEF2652L.IES
HEF265-2L-PL-U,HEF265-2L-PL-U,"32 Watt Rapid Start Medium Bi-Pin T8, 265mA, 48""",Two Lamp Fixture,Plate Glass,0,0,0,T8,32,64,80,277,37 lbs.,HEF2652L.IES
HEF430-2L-TM-A,HEF430-2L-TM-A,"34 Watt Rapid Start Medium Bi-Pin T12, 430mA, 48""",Two Lamp Fixture,Tempered Glass,0,0,0,T12,34,68,60,120,37 lbs.,HEF4302L.IES
HEF430-2L-PL-A,HEF430-2L-PL-A,"34 Watt Rapid Start Medium Bi-Pin T12, 430mA, 48""",Two Lamp Fixture,Plate Glass,0,0,0,T12,34,68,60,120,37 lbs.,HEF4302L.IES
HEF430-2L-TM-B,HEF430-2L-TM-B,"34 Watt Rapid Start Medium Bi-Pin T12, 430mA, 48""",Two Lamp Fixture,Tempered Glass,0,0,0,T12,34,68,60,236,37 lbs.,HEF4302L.IES
HEF430-2L-PL-B,HEF430-2L-PL-B,"34 Watt Rapid Start Medium Bi-Pin T12, 430mA, 48""",Two Lamp Fixture,Plate Glass,0,0,0,T12,34,68,60,236,37 lbs.,HEF4302L.IES
HEF430-2L-TM-C,HEF430-2L-TM-C,"34 Watt Rapid Start Medium Bi-Pin T12, 430mA, 48""",Two Lamp Fixture,Tempered Glass,0,0,0,T12,34,68,60,277,37 lbs.,HEF4302L.IES
HEF430-2L-PL-C,HEF430-2L-PL-C,"34 Watt Rapid Start Medium Bi-Pin T12, 430mA, 48""",Two Lamp Fixture,Plate Glass,0,0,0,T12,34,68,60,277,37 lbs.,HEF4302L.IES
HEF430-2L-TM-D,HEF430-2L-TM-D,"34 Watt Rapid Start Medium Bi-Pin T12, 430mA, 48""",Two Lamp Fixture,Tempered Glass,0,0,0,T12,34,68,60,220,37 lbs.,HEF4302L.IES
HEF430-2L-PL-D,HEF430-2L-PL-D,"34 Watt Rapid Start Medium Bi-Pin T12, 430mA, 48""",Two Lamp Fixture,Plate Glass,0,0,0,T12,34,68,60,220,37 lbs.,HEF4302L.IES
HEFT5HO-2L-TM-U,HEFT5HO-2L-TM-U,"54 Watt T5HO Miniature Bi-Pin 2 Lamp, 48""",Two Lamp Fixture,Tempered Glass,0,1,0,T5HO,54,108,80,277,41 lbs.,HEFT5HO4.IES
HEFT5HO-2L-PL-U,HEFT5HO-2L-PL-U,"54 Watt T5HO Miniature Bi-Pin 2 Lamp, 48""",Two Lamp Fixture,Plate Glass,0,1,0,T5HO,54,108,80,277,41 lbs.,HEFT5HO4.IES
HEF800-2L-TM-U,HEF800-2L-TM-U,"60 Watt, Rapid Start High Ouput Recessed Double Contact 800MA Lamps, 48""",Two Lamp Fixture,Tempered Glass,0,0,0,T8,60,240,80,277,37 lbs.,HEF8002L.IES
HEF800-2L-PL-U,HEF800-2L-PL-U,"60 Watt, Rapid Start High Ouput Recessed Double Contact 800MA Lamps, 48""",Two Lamp Fixture,Plate Glass,0,0,0,T8,60,240,80,277,37 lbs.,HEF8002L.IES
HEF265-3L-TM-U,HEF265-3L-TM-U,"32 Watt Rapid Start Medium Bi-Pin T8, 265mA, 48""",Three Lamp Fixture,Tempered Glass,1,0,0,T8,32,96,80,277,43 lbs.,HEF2653L.IES
HEF265-3L-PL-U,HEF265-3L-PL-U,"32 Watt Rapid Start Medium Bi-Pin T8, 265mA, 48""",Three Lamp Fixture,Plate Glass,1,0,0,T8,32,96,80,277,43 lbs.,HEF2653L.IES
HEF430-3L-TM-A,HEF430-3L-TM-A,"34 Watt Rapid Start Medium Bi-Pin 430mA Lamps, 48""",Three Lamp Fixture,Tempered Glass,1,0,0,T12,34,102,60,120,43 lbs.,HEF4303L.IES
HEF430-3L-PL-A,HEF430-3L-PL-A,"34 Watt Rapid Start Medium Bi-Pin 430mA Lamps, 48""",Three Lamp Fixture,Plate Glass,1,0,0,T12,34,102,60,120,43 lbs.,HEF4303L.IES
HEF430-3L-TM-C,HEF430-3L-TM-C,"34 Watt Rapid Start Medium Bi-Pin 430mA Lamps, 48""",Three Lamp Fixture,Tempered Glass,1,0,0,T12,34,102,60,277,43 lbs.,HEF4303L.IES
HEF430-3L-PL-C,HEF430-3L-PL-C,"34 Watt Rapid Start Medium Bi-Pin 430mA Lamps, 48""",Three Lamp Fixture,Plate Glass,1,0,0,T12,34,102,60,277,43 lbs.,HEF4303L.IES
HEFT5HO-3L-TM-U,HEFT5HO-3L-TM-U,"54 Watt T5HO Miniature Bi-Pin 2 Lamp, 48""",Three Lamp Fixture,Tempered Glass,0,0,1,T12,34,102,80,277,41 lbs.,HEFT5HO6.IES
HEFT5HO-3L-PL-U,HEFT5HO-3L-PL-U,"54 Watt T5HO Miniature Bi-Pin 2 Lamp, 48""",Three Lamp Fixture,Plate Glass,0,0,1,T12,34,102,80,277,41 lbs.,HEFT5HO6.IES
HEF800-3L-TM-U,HEF800-3L-TM-U,"60 Watt, Rapid Start High Ouput Recessed Double Contact 800MA Lamps, 48""",Three Lamp Fixture,Tempered Glass,1,0,0,T8,60,360,80,277,43 lbs.,HEF8003L.IES
HEF800-3L-PL-U,HEF800-3L-PL-U,"60 Watt, Rapid Start High Ouput Recessed Double Contact 800MA Lamps, 48""",Three Lamp Fixture,Plate Glass,1,0,0,T8,60,360,80,277,43 lbs.,HEF8003L.IES
